T1FD8 94941:414 SEGGER J-Link V6.30h Log File (0000ms, 1316862ms total)
T1FD8 94941:414 DLL Compiled: Mar 16 2018 18:02:51 (0000ms, 1316862ms total)
T1FD8 94941:414 Logging started @ 2018-07-28 20:13 (0000ms, 1316862ms total)
T1FD8 94941:414 JLINK_SetWarnOutHandler(...) (0000ms, 1316862ms total)
T1FD8 94941:414 JLINK_OpenEx(...)
Firmware: J-Link V9 compiled Mar  2 2018 17:07:57
Hardware: V9.10
S/N: 59103118
Feature(s): GDB
TELNET listener socket opened on port 19021WEBSRV 
Starting webserver (0125ms, 1316987ms total)
T1FD8 94941:414 WEBSRV Webserver running on local port 19080 (0125ms, 1316987ms total)
T1FD8 94941:414   returns O.K. (0125ms, 1316987ms total)
T1FD8 94941:540 JLINK_GetEmuCaps()  returns 0xB9FF7BBF (0000ms, 1316987ms total)
T1FD8 94941:540 JLINK_TIF_GetAvailable(...) (0001ms, 1316988ms total)
T1FD8 94941:541 JLINK_SetErrorOutHandler(...) (0000ms, 1316988ms total)
T1FD8 94941:541 JLINK_ExecCommand("ProjectFile = "C:\Users\Sergei\Documents\MK\ARM\Energy_Micro\AMW037\Client1\JLinkSettings.ini"", ...).   returns 0x00 (0001ms, 1316989ms total)
T1FD8 94941:542 JLINK_ExecCommand("Device = EFM32TG110F32", ...). Device "EFM32TG110F32" selected.  returns 0x00 (0002ms, 1316991ms total)
T1FD8 94941:544 JLINK_ExecCommand("DisableConnectionTimeout", ...).   returns 0x01 (0000ms, 1316991ms total)
T1FD8 94941:544 JLINK_GetHardwareVersion()  returns 0x16378 (0000ms, 1316991ms total)
T1FD8 94941:544 JLINK_GetDLLVersion()  returns 63008 (0000ms, 1316991ms total)
T1FD8 94941:544 JLINK_GetFirmwareString(...) (0000ms, 1316991ms total)
T1FD8 94941:544 JLINK_GetDLLVersion()  returns 63008 (0000ms, 1316991ms total)
T1FD8 94941:544 JLINK_GetCompileDateTime() (0000ms, 1316991ms total)
T1FD8 94941:544 JLINK_GetFirmwareString(...) (0000ms, 1316991ms total)
T1FD8 94941:544 JLINK_GetHardwareVersion()  returns 0x16378 (0000ms, 1316991ms total)
T1FD8 94941:544 JLINK_TIF_Select(JLINKARM_TIF_SWD)  returns 0x00 (0001ms, 1316992ms total)
T1FD8 94941:546 JLINK_SetSpeed(5000) (0000ms, 1316992ms total)
T1FD8 94941:546 JLINK_GetId() >0x10B TIF>Found SW-DP with ID 0x2BA01477 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x10B TIF>Found SW-DP with ID 0x2BA01477 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF>Scanning AP map to find all available APs >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>
 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>AP[1]: Stopped AP scan as end of AP map has been reachedAP[0]: AHB-AP (IDR: 0x24770011)Iterating through AP map to find AHB-AP to use >0x42 TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x42 TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>AP[0]: Core foundAP[0]: AHB-AP ROM base: 0xE00FF000 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF>
 >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>CPUID register: 0x412FC231. Implementer code: 0x41 (ARM)Found Cortex-M3 r2p1, Little endian. -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE0002000)FPUnit: 6 code (BP) slots and 2 literal slots -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_ReadMem(4 bytes @ 0xE000ED88)
 -- CPU_WriteMem(4 bytes @ 0xE000ED88) -- CPU_ReadMem(4 bytes @ 0xE000ED88) -- CPU_WriteMem(4 bytes @ 0xE000ED88)CoreSight components:ROMTbl[0] @ E00FF000 -- CPU_ReadMem(16 bytes @ 0xE00FF000) -- CPU_ReadMem(16 bytes @ 0xE000EFF0) -- CPU_ReadMem(16 bytes @ 0xE000EFE0)ROMTbl[0][0]: E000E000, CID: B105E00D, PID: 000BB000 SCS -- CPU_ReadMem(16 bytes @ 0xE0001FF0) -- CPU_ReadMem(16 bytes @ 0xE0001FE0)ROMTbl[0][1]: E0001000, CID: B105E00D, PID: 003BB002 DWT -- CPU_ReadMem(16 bytes @ 0xE0002FF0)
 -- CPU_ReadMem(16 bytes @ 0xE0002FE0)ROMTbl[0][2]: E0002000, CID: B105E00D, PID: 002BB003 FPB -- CPU_ReadMem(16 bytes @ 0xE0000FF0) -- CPU_ReadMem(16 bytes @ 0xE0000FE0)ROMTbl[0][3]: E0000000, CID: B105E00D, PID: 003BB001 ITM -- CPU_ReadMem(16 bytes @ 0xE00FF010) -- CPU_ReadMem(16 bytes @ 0xE0040FF0) -- CPU_ReadMem(16 bytes @ 0xE0040FE0)ROMTbl[0][4]: E0040000, CID: B105900D, PID: 003BB923 TPIU-Lite >0x0D TIF> >0x21 TIF>  returns 0x2BA01477 (0182ms, 1317174ms total)
T1FD8 94941:728 JLINK_GetDLLVersion()  returns 63008 (0000ms, 1317174ms total)
T1FD8 94941:728 JLINK_CORE_GetFound()  returns 0x30000FF (0000ms, 1317174ms total)
T1FD8 94941:728 JLINK_GetDebugInfo(0x100 = JLINKARM_ROM_TABLE_ADDR_INDEX) -- Value=0xE00FF000  returns 0x00 (0000ms, 1317174ms total)
T1FD8 94941:728 JLINK_GetDebugInfo(0x100 = JLINKARM_ROM_TABLE_ADDR_INDEX) -- Value=0xE00FF000  returns 0x00 (0000ms, 1317174ms total)
T1FD8 94941:728 JLINK_GetDebugInfo(0x101 = JLINKARM_DEBUG_INFO_ETM_ADDR_INDEX) -- Value=0x00000000  returns 0x00 (0001ms, 1317175ms total)
T1FD8 94941:729 JLINK_ReadMemEx(0xE0041FF0, 0x0010 Bytes, ..., Flags = 0x02000004) -- CPU_ReadMem(16 bytes @ 0xE0041FF0) - Data: 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00  returns 0x10 (0000ms, 1317175ms total)
T1FD8 94941:729 JLINK_GetDebugInfo(0x102 = JLINKARM_DEBUG_INFO_MTB_ADDR_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 1317175ms total)
T1FD8 94941:729 JLINK_GetDebugInfo(0x103 = JLINKARM_DEBUG_INFO_TPIU_ADDR_INDEX) -- Value=0xE0040000  returns 0x00 (0000ms, 1317175ms total)
T1FD8 94941:729 JLINK_GetDebugInfo(0x104 = JLINKARM_DEBUG_INFO_ITM_ADDR_INDEX) -- Value=0xE0000000  returns 0x00 (0000ms, 1317175ms total)
T1FD8 94941:729 JLINK_GetDebugInfo(0x105 = JLINKARM_DEBUG_INFO_DWT_ADDR_INDEX) -- Value=0xE0001000  returns 0x00 (0000ms, 1317175ms total)
T1FD8 94941:729 JLINK_GetDebugInfo(0x106 = JLINKARM_DEBUG_INFO_FPB_ADDR_INDEX) -- Value=0xE0002000  returns 0x00 (0000ms, 1317175ms total)
T1FD8 94941:729 JLINK_GetDebugInfo(0x107 = JLINKARM_DEBUG_INFO_NVIC_ADDR_INDEX) -- Value=0xE000E000  returns 0x00 (0000ms, 1317175ms total)
T1FD8 94941:730 JLINK_GetDebugInfo(0x10C = JLINKARM_DEBUG_INFO_DBG_ADDR_INDEX) -- Value=0xE000EDF0  returns 0x00 (0000ms, 1317175ms total)
T1FD8 94941:730 JLINK_GetDebugInfo(0x01 = Unknown) -- Value=0x00000000  returns 0x00 (0000ms, 1317175ms total)
T1FD8 94941:730 JLINK_ReadMemU32(0xE000ED00, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED00) - Data: 31 C2 2F 41  returns 0x01 (0000ms, 1317175ms total)
T1FD8 94941:730 JLINK_GetDebugInfo(0x10F = JLINKARM_DEBUG_INFO_HAS_CORTEX_M_SECURITY_EXT_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 1317175ms total)
T1FD8 94941:730 JLINK_SetResetType(JLINKARM_CM3_RESET_TYPE_NORMAL)  returns JLINKARM_CM3_RESET_TYPE_NORMAL (0000ms, 1317175ms total)
T1FD8 94941:730 JLINK_Reset() -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC)Reset: Halt core after reset via DEMCR.VC_CORERESET. >0x35 TIF>Reset: Reset device via AIRCR.SYSRESETREQ. -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000ED0C) >0x0D TIF> >0x28 TIF> -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running
 -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) (0067ms, 1317242ms total)
T1FD8 94941:797 JLINK_ReadReg(R15 (PC))  returns 0x00000138 (0000ms, 1317242ms total)
T1FD8 94941:797 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 1317242ms total)
T1FD8 94941:797 JLINK_Halt()  returns 0x00 (0001ms, 1317243ms total)
T1FD8 94941:798 JLINK_ReadMemU32(0xE000EDF0, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) - Data: 03 00 03 00  returns 0x01 (0000ms, 1317243ms total)
T1FD8 94941:798 JLINK_WriteU32(0xE000EDF0, 0xA05F0003) -- CPU_WriteMem(4 bytes @ 0xE000EDF0)  returns 0x00 (0001ms, 1317244ms total)
T1FD8 94941:799 JLINK_WriteU32(0xE000EDFC, 0x01000000) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0x00 (0001ms, 1317245ms total)
T1FD8 94941:800 JLINK_GetHWStatus(...)  returns 0x00 (0001ms, 1317246ms total)
T1FD8 94941:801 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)  returns 0x06 (0000ms, 1317246ms total)
T1FD8 94941:801 JLINK_GetNumBPUnits(Type = 0xF0)  returns 0x2000 (0000ms, 1317246ms total)
T1FD8 94941:801 JLINK_GetNumWPUnits()  returns 0x04 (0000ms, 1317246ms total)
T1FD8 94941:801 JLINK_GetSpeed()  returns 0xFA0 (0000ms, 1317246ms total)
T1FD8 94941:801 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) - Data: 00 00 00 00  returns 0x01 (0000ms, 1317246ms total)
T1FD8 94941:801 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) - Data: 00 00 00 00  returns 0x01 (0001ms, 1317247ms total)
T1FD8 94941:802 JLINK_WriteMemEx(0xE0001000, 0x001C Bytes, ..., Flags = 0x02000004) - Data: 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ... -- CPU_WriteMem(28 bytes @ 0xE0001000)  returns 0x1C (0002ms, 1317249ms total)
T1FD8 94941:804 JLINK_ReadReg(R15 (PC))  returns 0x00000138 (0000ms, 1317249ms total)
T1FD8 94941:804 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 1317249ms total)
T1FD8 94941:872 JLINK_SetResetType(JLINKARM_CM3_RESET_TYPE_NORMAL)  returns JLINKARM_CM3_RESET_TYPE_NORMAL (0000ms, 1317249ms total)
T1FD8 94941:872 JLINK_Reset() -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)Reset: Halt core after reset via DEMCR.VC_CORERESET. >0x35 TIF>Reset: Reset device via AIRCR.SYSRESETREQ. -- CPU_WriteMem(4 bytes @ 0xE000ED0C) >0x0D TIF> >0x28 TIF> -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000)
 -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) (0072ms, 1317321ms total)
T1FD8 94941:945 JLINK_ReadReg(R15 (PC))  returns 0x00000138 (0000ms, 1317321ms total)
T1FD8 94941:945 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 1317321ms total)
T1FD8 94941:946 JLINK_ReadMemEx(0x00000138, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(128 bytes @ 0x00000100) -- Updating C cache (128 bytes @ 0x00000100) -- Read from C cache (60 bytes @ 0x00000138) - Data: 08 48 00 47 FE E7 FE E7 FE E7 FE E7 FE E7 FE E7 ...  returns 0x3C (0001ms, 1317322ms total)
T1FD8 94943:563 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 1317322ms total)
T1FD8 94943:563 JLINK_ReadReg(R1)  returns 0x00000000 (0000ms, 1317322ms total)
T1FD8 94943:563 JLINK_ReadReg(R2)  returns 0x00000900 (0000ms, 1317322ms total)
T1FD8 94943:563 JLINK_ReadReg(R3)  returns 0x04C11DB7 (0000ms, 1317322ms total)
T1FD8 94943:563 JLINK_ReadReg(R4)  returns 0x00000000 (0000ms, 1317322ms total)
T1FD8 94943:563 JLINK_ReadReg(R5)  returns 0x00000000 (0000ms, 1317322ms total)
T1FD8 94943:563 JLINK_ReadReg(R6)  returns 0x00000000 (0001ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(R7)  returns 0x00000000 (0000ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(R9)  returns 0x200001DC (0000ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(R10)  returns 0x00000000 (0000ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(R11)  returns 0x00000000 (0000ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(R13 (SP))  returns 0x200002C0 (0000ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(R14)  returns 0xFFFFFFFF (0000ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(R15 (PC))  returns 0x00000138 (0000ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(MSP)  returns 0x200002C0 (0000ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(PSP)  returns 0x20001000 (0000ms, 1317323ms total)
T1FD8 94943:564 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 1317323ms total)
T1FD8 94943:570 JLINK_ReadMemEx(0x2000000C, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x2000000C) - Data: 40 00 00 D3 58 40 64 1E FA D1 49 1C 52 1E 00 2A ...  returns 0x20 (0001ms, 1317324ms total)
T1B6C 94943:599 JLINK_ReadMemEx(0x00000138, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x00000138) - Data: 08 48  returns 0x02 (0000ms, 1317324ms total)
T1B6C 94943:599 JLINK_SetBPEx(Addr = 0x000006E8, Type = 0xFFFFFFF2)  returns 0x00000001 (0000ms, 1317324ms total)
T1B6C 94943:599 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) -- CPU_WriteMem(4 bytes @ 0xE0001004) (0004ms, 1317328ms total)
T1B6C 94943:703 JLINK_IsHalted()  returns TRUE (0002ms, 1317330ms total)
T1B6C 94943:705 JLINK_Halt()  returns 0x00 (0000ms, 1317328ms total)
T1B6C 94943:705 JLINK_IsHalted()  returns TRUE (0000ms, 1317328ms total)
T1B6C 94943:705 JLINK_IsHalted()  returns TRUE (0000ms, 1317328ms total)
T1B6C 94943:705 JLINK_IsHalted()  returns TRUE (0000ms, 1317328ms total)
T1B6C 94943:705 JLINK_ReadReg(R15 (PC))  returns 0x000006E8 (0000ms, 1317328ms total)
T1B6C 94943:705 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 1317328ms total)
T1B6C 94943:705 JLINK_ClrBPEx(BPHandle = 0x00000001)  returns 0x00 (0000ms, 1317328ms total)
T1B6C 94943:705 JLINK_ReadMemU32(0xE000ED30, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED30) - Data: 02 00 00 00  returns 0x01 (0001ms, 1317329ms total)
T1B6C 94943:706 JLINK_ReadMemU32(0xE0001028, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001028) - Data: 00 00 00 00  returns 0x01 (0001ms, 1317330ms total)
T1B6C 94943:707 JLINK_ReadMemU32(0xE0001038, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001038) - Data: 00 02 00 00  returns 0x01 (0000ms, 1317330ms total)
T1B6C 94943:707 JLINK_ReadMemU32(0xE0001048, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001048) - Data: 00 00 00 00  returns 0x01 (0001ms, 1317331ms total)
T1B6C 94943:708 JLINK_ReadMemU32(0xE0001058, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001058) - Data: 00 00 00 00  returns 0x01 (0000ms, 1317331ms total)
T1B6C 94943:708 JLINK_ReadReg(R0)  returns 0x000006E9 (0000ms, 1317331ms total)
T1B6C 94943:708 JLINK_ReadReg(R1)  returns 0x00000000 (0000ms, 1317331ms total)
T1B6C 94943:708 JLINK_ReadReg(R2)  returns 0x00000900 (0000ms, 1317331ms total)
T1B6C 94943:708 JLINK_ReadReg(R3)  returns 0x04C11DB7 (0001ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(R4)  returns 0x00000000 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(R5)  returns 0x00000000 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(R6)  returns 0x00000000 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(R7)  returns 0x00000000 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(R9)  returns 0x200001DC (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(R10)  returns 0x00000000 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(R11)  returns 0x00000000 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(R13 (SP))  returns 0x200002C0 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(R14)  returns 0xFFFFFFFF (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(R15 (PC))  returns 0x000006E8 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(MSP)  returns 0x200002C0 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(PSP)  returns 0x20001000 (0000ms, 1317332ms total)
T1B6C 94943:709 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 1317332ms total)
T1FD8 94943:710 JLINK_ReadMemEx(0x200002B0, 0x0008 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(8 bytes @ 0x200002B0) - Data: 6F 73 65 0D 0A 0D 0A 00  returns 0x08 (0001ms, 1317333ms total)
T1FD8 94943:711 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001004) - Data: 08 00 00 00  returns 0x01 (0001ms, 1317334ms total)
T1FD8 94943:712 JLINK_ReadMemEx(0x2000000C, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x2000000C) - Data: 40 00 00 D3 58 40 64 1E FA D1 49 1C 52 1E 00 2A ...  returns 0x20 (0001ms, 1317335ms total)
T1FD8 94943:713 JLINK_ReadMemEx(0x000006E8, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(128 bytes @ 0x000006C0) -- Updating C cache (128 bytes @ 0x000006C0) -- Read from C cache (60 bytes @ 0x000006E8) - Data: 1C B5 26 A1 03 C9 CD E9 00 01 FF F7 A1 FD FF F7 ...  returns 0x3C (0001ms, 1317336ms total)
T1B6C 94944:511 JLINK_ReadMemEx(0x000006E8, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x000006E8) - Data: 1C B5  returns 0x02 (0000ms, 1317336ms total)
T1B6C 94944:511 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) (0003ms, 1317339ms total)
T1B6C 94944:614 JLINK_IsHalted()  returns FALSE (0000ms, 1317339ms total)
T1B6C 94944:714 JLINK_IsHalted()  returns FALSE (0000ms, 1317339ms total)
T1B6C 94944:814 JLINK_IsHalted()  returns FALSE (0000ms, 1317339ms total)
T1B6C 94944:914 JLINK_IsHalted()  returns FALSE (0000ms, 1317339ms total)
T1B6C 94945:014 JLINK_IsHalted()  returns FALSE (0000ms, 1317339ms total)
T1B6C 94945:114 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001004) - Data: 49 67 80 00  returns 0x01 (0001ms, 1317340ms total)
T1FD8 94945:115 JLINK_ReadMemEx(0x2000000C, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x2000000C) - Data: 40 32 0D 74 20 77 6C 20 6E 20 73 0D 52 1E 00 2A ...  returns 0x20 (0001ms, 1317341ms total)
T1B6C 94945:118 JLINK_IsHalted()  returns FALSE (0001ms, 1317342ms total)
T1B6C 94945:219 JLINK_IsHalted()  returns FALSE (0000ms, 1317341ms total)
T1B6C 94945:319 JLINK_IsHalted()  returns FALSE (0000ms, 1317341ms total)
T1B6C 94945:420 JLINK_IsHalted()  returns FALSE (0000ms, 1317341ms total)
T1B6C 94945:520 JLINK_IsHalted()  returns FALSE (0000ms, 1317341ms total)
T1B6C 94945:620 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 49 67 80 00  returns 0x01 (0000ms, 1317341ms total)
T1FD8 94945:620 JLINK_ReadMemEx(0x2000000C, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x2000000C) - Data: 40 32 0D 74 20 77 6C 20 6E 20 73 0D 52 1E 00 2A ...  returns 0x20 (0001ms, 1317342ms total)
T1B6C 94945:621 JLINK_IsHalted()  returns FALSE (0001ms, 1317343ms total)
T1B6C 94945:722 JLINK_IsHalted()  returns FALSE (0000ms, 1317342ms total)
T1B6C 94945:822 JLINK_IsHalted()  returns FALSE (0000ms, 1317342ms total)
T1B6C 94945:922 JLINK_IsHalted()  returns FALSE (0001ms, 1317343ms total)
T1B6C 94946:023 JLINK_IsHalted()  returns FALSE (0001ms, 1317343ms total)
T1B6C 94946:124 JLINK_IsHalted()  returns FALSE (0001ms, 1317343ms total)
T1B6C 94946:225 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 49 67 80 00  returns 0x01 (0000ms, 1317342ms total)
T1FD8 94946:227 JLINK_ReadMemEx(0x2000000C, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x2000000C) - Data: 40 32 0D 74 20 77 6C 20 6E 20 73 0D 52 1E 00 2A ...  returns 0x20 (0002ms, 1317344ms total)
T1B6C 94946:229 JLINK_IsHalted()  returns FALSE (0001ms, 1317345ms total)
T1B6C 94946:330 JLINK_IsHalted()  returns FALSE (0000ms, 1317344ms total)
T1B6C 94946:431 JLINK_IsHalted()  returns FALSE (0001ms, 1317345ms total)
T1B6C 94946:532 JLINK_IsHalted()  returns FALSE (0001ms, 1317345ms total)
T1B6C 94946:633 JLINK_IsHalted()  returns FALSE (0001ms, 1317345ms total)
T1B6C 94946:734 JLINK_IsHalted()  returns FALSE (0000ms, 1317344ms total)
T1B6C 94946:834 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 49 67 80 00  returns 0x01 (0000ms, 1317344ms total)
T1FD8 94946:834 JLINK_ReadMemEx(0x2000000C, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x2000000C) - Data: 40 32 0D 74 20 77 6C 20 6E 20 73 0D 52 1E 00 2A ...  returns 0x20 (0001ms, 1317345ms total)
T1B6C 94946:835 JLINK_IsHalted()  returns FALSE (0001ms, 1317346ms total)
T1B6C 94946:936 JLINK_IsHalted()  returns FALSE (0000ms, 1317345ms total)
T1B6C 94947:036 JLINK_IsHalted()  returns FALSE (0000ms, 1317345ms total)
T1B6C 94947:136 JLINK_IsHalted()  returns FALSE (0000ms, 1317345ms total)
T1B6C 94947:236 JLINK_IsHalted()  returns FALSE (0000ms, 1317345ms total)
T1B6C 94947:336 JLINK_IsHalted()  returns FALSE (0000ms, 1317345ms total)
T1B6C 94947:436 JLINK_ReadMemU32(0xE0001004, 0x0001 Items, ...) - Data: 49 67 80 00  returns 0x01 (0000ms, 1317345ms total)
T1FD8 94947:447 JLINK_ReadMemEx(0x2000000C, 0x0020 Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(32 bytes @ 0x2000000C) - Data: 40 32 0D 74 20 77 6C 20 6E 20 73 0D 52 1E 00 2A ...  returns 0x20 (0001ms, 1317346ms total)
T1B6C 94947:448 JLINK_IsHalted()  returns FALSE (0001ms, 1317347ms total)
T1B6C 94947:549 JLINK_Halt()  returns 0x00 (0003ms, 1317349ms total)
T1B6C 94947:552 JLINK_IsHalted()  returns TRUE (0000ms, 1317349ms total)
T1B6C 94947:553 JLINK_IsHalted()  returns TRUE (0000ms, 1317349ms total)
T1B6C 94947:553 JLINK_IsHalted()  returns TRUE (0000ms, 1317349ms total)
T1B6C 94947:553 JLINK_ReadReg(R15 (PC))  returns 0x00000724 (0000ms, 1317349ms total)
T1B6C 94947:553 JLINK_ReadReg(XPSR)  returns 0x41000000 (0000ms, 1317349ms total)
T1B6C 94947:553 JLINK_ReadMemU32(0xE000ED30, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED30) - Data: 01 00 00 00  returns 0x01 (0001ms, 1317350ms total)
T1B6C 94947:554 JLINK_ReadMemU32(0xE0001028, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001028) - Data: 00 00 00 00  returns 0x01 (0001ms, 1317351ms total)
T1B6C 94947:555 JLINK_ReadMemU32(0xE0001038, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001038) - Data: 00 02 00 00  returns 0x01 (0001ms, 1317352ms total)
T1B6C 94947:556 JLINK_ReadMemU32(0xE0001048, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001048) - Data: 00 00 00 00  returns 0x01 (0001ms, 1317353ms total)
T1B6C 94947:557 JLINK_ReadMemU32(0xE0001058, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001058) - Data: 00 00 00 00  returns 0x01 (0000ms, 1317353ms total)
T1FD8 94948:251 JLINK_Close() -- CPU_ReadMem(4 bytes @ 0xE0001000) >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> (0028ms, 1317381ms total)
T1FD8 94948:251  (0028ms, 1317381ms total)
T1FD8 94948:251 Closed (0028ms, 1317381ms total)
